DRYWALL FINISHER (NOC 7284) 

LG Drywalling Inc. 
1432 Seaview Drive 

Mississauga, Ontario L5J 1X5 

Job Type: Permanent, Full Time, Weekend, Day, Night and Evening

Salary: $34.00 Hourly for 35 hours per week 
Anticipated Start Date: As soon as possible 
Location: Toronto, Ontario (2 vacancy)
We are a small and fast-growing drywall company providing different services to residential, industrial, and commercial builders. We are currently looking to hire a Drywall Finisher with experience in this fast-growing trade. 

POSITION SUMMARY:
The Drywall Finisher will be responsible for the installation of steel stud frames and drywall and the finishing of drywall sheets (tape and plaster) in residential, industrial and commercial establishments. 

MAJOR RESPONSIBILITIES: 

· Read and interpret drawings and specifications to lead the installation of metal stud framing and furring for interior drywall or plaster walls, using hand and power tools.

· Determine insulation requirements and select type of insulation required 

· Measure and cut insulating material to required dimensions using hand and power tools.

· Apply insulation using spraying, blowing, pasting, strapping, taping and other application and installation methods

· Fit insulation around obstructions and between studs and joists

· Measure, cut and fit drywall sheets for installation

· Position and secure sheets to metal or wooden studs or joists

· Tape and finish drywall sheets using hand and automatic taping tools

QUALIFICATIONS/SKILLS REQUIRED:

· Education: Completion of high school, some college/CEGEP/vocational or technical 

      training.

· Experience: 3 years of work experience as a drywall finisher.
· Languages: Speak English, Read English, Write English 

HOW TO APPLY:

By email: hrlgdrywall@gmail.com
LG Drywalling Inc. is committed to diversity and equity; persons from underrepresented groups are encouraged to apply. We welcome applications from everyone in respect of gender, ethnic groups, youth, newcomers and person with disabilities.[image: image1]
