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Name                                                                 Samuel Barnes
Residential   Address                                         G38 Tarkwa
Postal Address                                                   Panafrican Mining service 
E-mail Address                                                 fatubarnes4040@gmail.com 
Date of Birth                                                     10th January, 1980
Profession                                                          Heavy-Duty Mechanic 
Marital Status                                                    Married
Nationality                                                        Ghanaian
Telephone number                                            00233275581230 /00233505810554
EDUCATIONAL BACKGROUND
Institution                                                         Cape coast polytechnic
Year                                                                  November /December 1999/2000
Certificate                                                         Higher National Diploma in Mech Eng
Institution                                                         University Of Mines And Technology  
Year                                                                  August 2004/2005
Certificate                                                         Maintenanace/Management
Institution                                                         Suhum Sec/tech school
Year                                                                  Feb 1995-Aug 1998
Certificate                                                         Metal work
PROFESSIONAL COMPETENCIES
Name of Company                                             Panafrican Mining Ghana Komastu
Year                                                                   April 2012
Course                                                               greasing system level 1&2
Name of Company                                            Panafrican Mining Ghana Komastu
Year                                                                  October, 2013
Course                                                               Report Writing/Contamination control
Name of company                                             Kanu equipment liberia
Year                                                                   June 2016
Course                                                               Basic electrics 
	
WORKING EXPERIENCIES
NAME OF COMPANY                                          Liebherr mining Ghana
JOB TITLE                                                             Heavy-duty Mechanic (fieldservice)
YEAR                                                                     March 2008-June 2012
SERVICE:    change of engine oil filters, engine oil, hydraulic oil filters, air filters, transmission oil filters check coolantlevel, hydraulicoil and transmission oil and top up respectively if necessary.Inspect frame and body for cracks and call welders to weld if cracks are found. Inspect hydraulic and coolant hose for leaks, check lose bolt and nuts, check pressures on torque convertor, transmission slag adjustors (front and rear)

MAJOR COMPONENT CHANGE OUT:    torque convertor (TC), transmission, engine, telescopic suspension, a frame bearing, bucket, hoist cylinder and tilt cylinder. Striping of excavator , the boom, counter weight, carbine radiator, control block, slew ring track, central guide, engine etc.
Trouble shooting:
1. Continuous oil shortage: Piston oil ring worn out oil filter base seal and gasket worn out or harden.Remove filter mounting and replace worn out seal and gasket.
1. Engine low performance: check air filter for debris if necessary change. Open engine covers and check valve clearance or damage component.

Ineffective breaking: check pressures on slag adjustor (front and rear) or main filter which supply hydraulic oil scavenge pump and the brakes (680:28), if not up to the manufacture recommendation adjust relief valve. After adjustment and pressures are not correct then change pressures relief valve.         

1. Implement not lifting, check working pump pressures, check pilot pressures, if not correct then check relieve and adjust or change completely.

1. Engine difficult starting, check battery positive and negative cables, if in place then check fuel lines for leakages and fuel filters for debris. Change fuel filter if clogged and fuel hose if found leaking.

TOOLS 
Spanners (combinations)
Impact
Puller
Hammer
Pneumatic jack
Hydraulic jack
Come along
Chain
Ply bar
Lifting sling
NAME OF COMPANY 				  Mantrac Ghana  Limited CAT
JOB TITLE					              Duty Mechanic (field service )
YEAR						             August 2012-January 2015
RESPONSIBILITIES	
SERVICE AND MAINTENANCE: Cary out preventive service at given period of time (250, 500, 1000 hours). Draining and replacement of engine oil change of air, fuel and oil filters. Taking oil samples, check coolant level, hydraulic oil level, Replacing of O - ring or hoses incase of leakages. Inspection of grease hose, grease injectors. After all jobs are done, run the engine and ensure proper working condition. Check body and frame for crack if any inform welders.

Engine Overhauling 
Dismantling of engine: Removing electrical hanners, pipes, engine covers, startor, alternator, flywheel enclose cylinder heard bolt and remove cylinder heard for damage, check valve seat, valve heard, valve spring, valve tappet, piston rings, connecting rod bearing, crankshaft main bearings and camshaft. All these checks and inspections should be done after all engine components or parts have been cleaned. Replace worn out bushes, bearings and damage component like piston ring, crankshaft, piston, cylinder liners, grinding of valves, change gasket etc. check for wear on crankshaft, main cap, connecting rod ends. If turbocharger is leaking replace or change seal, change seal, bearings and trust washers.

Under carriage
Inspections of excessive wear on sprocket, down and upper rollers, track pads track links. If worn out replacewith a new component. Leakage on track tensioned and driving motors. Check for burst hose and leakages on driving motors. Check for crakes on track frame, if any in form welders. Check worn out ripper tips.

Hydraulic problem:
Check pressure on machine; If pressure are not ok inspect high pressure filters if clogged replace. Dismantling, resealing and rebuilding of hydraulic cylinders. Replacement of oil seals, wiper seals, backup seal and O ring, heck pressure again if high reduce or adjust to manufactures specification. Carry out hydraulic tune up.

MACHINE WORK 
Komastu  excavators                                    PC200LC-7,PC400LC-7,D65PX-12               Komastu dumptruck                                     HD785-7,HD785-5,HM400-1     
Caterpillar Excavator                                      330CL AND 330BL
Dump Truck			                         777D, 777F, 785C
Loader				                         992K, 992G
Dozer				                         D10, D8
Caterpillar Engines                                          C27,C32,C3512,C3508
Liebherr excavator                                           994B,994/200,9350,9250,944
                                                                                   
                                                          
TOOLS FOR WORK
High Torque 
Torque Wrench
Torque Multiplier 
 Mallet Hammer
Dial Grinder
Hand Drill Machine
High Torque Head (23510)
Track Press
Press Motor
Spanner
Screw Driver
Shackle
Eye Bolt
Chain
Scraper
Files
Inner Pack
COMPANY                                        KANU EQUIPMENT  (Liberia)
JOB TITLE                                         Heavyduty Mechanic (SUPERVISOR)
YEAR                                                  Nov 2015- January 2018(EXPATRIATE )                
RESPONSIBILITIES
SERVICING: Draining and replacement of engine oil. Checks for brake efficiency, inspection of fan, alternator, timing belts. Tighten of loose bolts and change of damage bolts, crack checks on chassis. Inspection of coolant level,  carry out troble shooting ,use stimatic to trace fault ,do component change out and rebuilt of mechaine2015
MACHINE ASSEMBLING AND COMP0NENT REBUILD 2012
Assembly of excavators, dump truck and components rebuild like
Final drives 
Pump drive
TV
Hydraulic cylinders
Kanu Equipment Liberia
Tools for work
Spanners
Hammer
Chain
Inner Pack
Shackle
High torque
Track press
REFEREES
Peter   
MANAGER KANU EQUIPMENT LIBERIA
Cell +231888380563

Ketu Nuhu
Filed Service Supervisor | Mantrac Ghana | Newmont-Akyem
Cell +233 (0) 244 367544 

                                               




The Human Resource Manager


Dear sir 


       

APPLICATION FOR EMPLOYMENT AS MECHANIC SUPERVISOR 



I wish to apply for the position mentioned above in your highly esteem company.

I am a young man of Thirty-two (39) years of age with thirteen years working experience for the mentioned post.

I am dedicated and hardworking, ready to promote the goals of your company when I am given the opportunity.

I promise to abide by the rules and regulations governing the company and discharge my duties as a worker.

Attached are copies of Certificate, Curriculum Vitae for your perusal.

I hope my humble application will be given a favourable response from your highly office.


Thank you. 

Yours faithfully,
Samuel Barnes






